| Fall & Winter Commercial HVAC Maintenance Checklist |
| --- |

| **INSPECTION DATE:** |  | **TECHNICIAN:** |  |
| --- | --- | --- | --- |

| ▢ | Clean or replace filters. |
| --- | --- |

| ▢ | Inspect burner assembly. |
| --- | --- |

| ▢ | Check heat exchanger and other heating elements. |
| --- | --- |

| ▢ | Check for carbon monoxide or gas leaks in heating elements. |
| --- | --- |

| ▢ | Inspect electrical connections for frays or damage. |
| --- | --- |

| ▢ | Lubricate motor bearings and all moving parts. |
| --- | --- |

| ▢ | Inspect belts for damage or fraying. |
| --- | --- |

| ▢ | Check drains for blockages. |
| --- | --- |

| ▢ | Check gas pressure. |
| --- | --- |

| ▢ | Test thermostats. |
| --- | --- |

| ▢ | Test and check heat pump. |
| --- | --- |

| ▢ | Check ductwork and vents. |
| --- | --- |

| ▢ | Clean and check flue system. |
| --- | --- |

| ▢ | Check flue system’s attachment to the furnace. |
| --- | --- |

| **COMMENTS:** | | | |
| --- | --- | --- | --- |
|  | | | |