| Spring/Summer External Property Maintenance Checklist |
| --- |

| **INSPECTION DATE:** |  | **TECHNICIAN:** |  |
| --- | --- | --- | --- |

| ▢ | Inspect the roof for damage and debris. |
| --- | --- |

| ▢ | Inspect doors and windows and ensure sealant is intact. |
| --- | --- |

| ▢ | Put in or inspect window screens; check for holes and tears. |
| --- | --- |

| ▢ | Clear debris from exterior vents and clean if needed. |
| --- | --- |

| ▢ | Clear debris from gutters. |
| --- | --- |

| ▢ | Inspect outdoor component of HVAC unit. |
| --- | --- |

| ▢ | Check for cracks in sidewalks and parking lots. |
| --- | --- |

| ▢ | Trim trees that are overgrown, threatening property line, or too close to the building. |
| --- | --- |

| ▢ | Ensure all outdoor lighting fixtures are working correctly (adjust auto-on/off time if necessary). |
| --- | --- |

| ▢ | Make arrangements to begin weekly external tasks (mowing and lawn care, gardening, etc.). |
| --- | --- |

| **COMMENTS:** | | | |
| --- | --- | --- | --- |
|  | | | |