| Window Inspection Checklist |
| --- |

| **INSPECTION DATE:** |  | **TECHNICIAN:** |  |
| --- | --- | --- | --- |

| ▢ | Remove grime and debris from window sills. |
| --- | --- |

| ▢ | Check the interior and exterior finishes—peeling or water stains may indicate a leak, which means that they may need to be resealed or replaced. |
| --- | --- |

| ▢ | Check all locks and knobs to ensure they work properly. |
| --- | --- |

| ▢ | Add a non-oily lubricant to any windows that are sliding or sticking. |
| --- | --- |

| ▢ | Replace any windows that are damaged or do not stay open or closed properly. |
| --- | --- |

| **COMMENTS:** | | | |
| --- | --- | --- | --- |
|  | | | |